---Overview---

This code was developed in order to quantitatively map the variation of color with depth given a core log. Specifically the application maps the true averaged color with depth along with its corresponding redness-greeness, luminosity and yellowness-blueness. The code then plots this data in such a way that these four pieces of data can easily be compared side by side.

---Notes---

This code utilizes:
1) the image processing toolbox of Matlab
2) a colorspace conversion code that was developed by Pascal Getreuer 
	http://www.math.ucla.edu/~getreuer/colorspace.html

---Instructions---
1) Load images into a subfolder of the "Images" folder. If analyzing more than one well it will be useful to name the well image folders with consistency for instance "well_1", "well_2", etc.
	⁃	 It is important to name the well images numerically with increasing depth given a higher number such as d1.jpg, d2.jpg,d3.jpg etc
	⁃	the code was developed to support JPG images but the file format can easily be changed in the code

2) In the matlab code total_project.m you may specify the well name and the depths at which each picture was taken. 

3) Run the code and check out the plot it produces

---As packaged---

The code is set up to run through one well, specifically well 14 from the angelo coast range reserve. In order for it to loop through a series of wells the code will need to be modified slightly.